(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (title_block
    (title " \"XSE SDLogger")
    (date "2021-05-29")
    (rev "1.3")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (pcbplotparams
      (layerselection 0x0015054_fffffffe)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror true)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C5-Pad2)")
  (net 4 "Net-(C6-Pad2)")
  (net 5 "Net-(C7-Pad2)")
  (net 6 "Net-(C8-Pad2)")
  (net 7 "Net-(D1-Pad2)")
  (net 8 "Net-(D2-Pad2)")
  (net 9 "Net-(J1-Pad2)")
  (net 10 "Net-(J1-Pad3)")
  (net 11 "Net-(J2-Pad1)")
  (net 12 "Net-(J2-Pad2)")
  (net 13 "Net-(J2-Pad3)")
  (net 14 "Net-(J3-Pad1)")
  (net 15 "Net-(J3-Pad2)")
  (net 16 "Net-(J4-Pad1)")
  (net 17 "Net-(J4-Pad2)")
  (net 18 "Net-(J5-Pad1)")
  (net 19 "Net-(J5-Pad2)")
  (net 20 "Net-(J5-Pad3)")
  (net 21 "Net-(J5-Pad4)")
  (net 22 "Net-(R1-Pad1)")
  (net 23 "Net-(R2-Pad1)")
  (net 24 "Net-(R3-Pad2)")
  (net 25 "Net-(U1-Pad13)")
  (net 26 "Net-(U1-Pad14)")
  (net 27 "Net-(U1-Pad15)")
  (net 28 "Net-(U1-Pad16)")
  (net 29 "Net-(U1-Pad22)")
  (net 30 "Net-(U1-Pad23)")
  (net 31 "Net-(U1-Pad24)")
  (net 32 "Net-(U1-Pad25)")
  (net 33 "Net-(U1-Pad26)")
  (net 34 "Net-(U1-Pad30)")
  (net 35 "Net-(U1-Pad31)")
  (net 36 "Net-(U1-Pad32)")
  (net 37 "Net-(U1-Pad33)")
  (net 38 "Net-(U1-Pad42)")
  (net 39 "Net-(U1-Pad43)")
  (net 40 "Net-(U2-Pad4)")
  (net 41 "Net-(J6-Pad10)")
  (net 42 "Net-(J6-Pad1)")
  (net 43 "Net-(J6-Pad2)")
  (net 44 "Net-(J6-Pad8)")
  (net 45 "GND")
  (net 46 "VIN")
  (net 47 "+3V3")
  (footprint "xse-sdlogger:Socket_Strip_Straight_1x03_Pitch2.54mm" (layer "F.Cu")
    (at 133.7074 91.903)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x03_Female" (at 0 7.41) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.33) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(J3-Pad1)"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(J3-Pad2)"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 45 "GND"))
    (model "${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.54mm.wrl"
      (offset (xyz 0 -2.539999962 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (footprint "xse-sdlogger:Socket_Strip_Straight_1x04_Pitch2.54mm" (layer "F.Cu")
    (at 164.1874 107.133)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x04_Female" (at 0 9.95) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.33) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(J4-Pad1)"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(J4-Pad2)"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 47 "+3V3"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 45 "GND"))
    (model "${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x04_Pitch2.54mm.wrl"
      (offset (xyz 0 -3.809999943 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (footprint "xse-sdlogger:Socket_Strip_Straight_1x05_Pitch2.54mm" (layer "F.Cu")
    (at 164.1874 91.893)
    (descr "Through hole straight socket strip, 1x05, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x05 2.54mm single row")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x05_Female" (at 0 12.49) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.33) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(J5-Pad1)"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(J5-Pad2)"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(J5-Pad3)"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(J5-Pad4)"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 45 "GND"))
    (model "${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x05_Pitch2.54mm.wrl"
      (offset (xyz 0 -5.079999924 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (footprint "xse-sdlogger:Socket_Strip_Straight_1x06_Pitch2.54mm" (layer "F.Cu")
    (at 143.08986 114.763 90)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Female" (at 0 15.03 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.33 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(J2-Pad1)"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(J2-Pad2)"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(J2-Pad3)"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(C1-Pad2)"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 47 "+3V3"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 45 "GND"))
    (model "${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.54mm.wrl"
      (offset (xyz 0 -6.349999905 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (footprint "xse-sdlogger:LED_0805_HandSoldering" (layer "F.Cu")
    (at 156.425 91.0336)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "D1" (at 2.071 1.6764) (layer "F.SilkS"))
    (fp_text value "BLUE" (at 0 1.75) (layer "F.Fab") hide)
    (pad "1" smd rect (at -1.35 0) (size 1.5 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "GND"))
    (pad "2" smd rect (at 1.35 0) (size 1.5 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(D1-Pad2)"))
    (model "${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xse-sdlogger:Socket_Strip_Straight_1x06_Pitch2.54mm" (layer "F.Cu")
    (at 133.7074 102.063)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Female" (at 0 15.03) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.33) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(C1-Pad1)"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(J1-Pad2)"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(J1-Pad3)"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 46 "VIN"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 45 "GND"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 45 "GND"))
    (model "${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.54mm.wrl"
      (offset (xyz 0 -6.349999905 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (footprint "xse-sdlogger:microSD_Card_Reverse_Yamaichi_PSJ-008-2003-1" (layer "F.Cu")
    (at 148.9473 102.5017 90)
    (descr "http://katalog.we-online.de/em/datasheet/693072010801.pdf")
    (tags "Micro SD Wuerth Wurth Würth")
    (attr smd)
    (fp_text reference "J6" (at 13.11912 0.00118 180) (layer "F.SilkS") hide)
    (fp_text value "PJS-008-2003-1" (at 3.429 11.8872 270) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.9746 0 270) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 -3.55 90) (size 1.2 1.2) (drill 0.6) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 0 4 90) (size 1.2 1.2) (drill 0.6) (layers "*.Mask"))
    (pad "1" smd rect (at -5.8 2.6 90) (size 1.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "Net-(J6-Pad1)"))
    (pad "2" smd rect (at -5.8 1.5 90) (size 1.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "Net-(J6-Pad2)"))
    (pad "3" smd rect (at -5.8 0.4 90) (size 1.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(J2-Pad1)"))
    (pad "4" smd rect (at -5.8 -0.7 90) (size 1.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C5-Pad2)"))
    (pad "5" smd rect (at -5.8 -1.8 90) (size 1.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(J2-Pad3)"))
    (pad "6" smd rect (at -5.8 -2.9 90) (size 1.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "GND"))
    (pad "7" smd rect (at -5.8 -4 90) (size 1.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(J2-Pad2)"))
    (pad "8" smd rect (at -5.8 -5.1 90) (size 1.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(J6-Pad8)"))
    (pad "9" smd rect (at -5.8 -6.2 90) (size 1.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "GND"))
    (pad "10" smd rect (at 4.4 -7.4 90) (size 0.8 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(J6-Pad10)"))
    (pad "11" smd rect (at -4.15 -7.585 90) (size 3.1 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "GND"))
    (pad "11" smd rect (at -3.02286 7.5 90) (size 3.65 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "GND"))
    (pad "11" smd rect (at 7.35 -7.5 90) (size 3.5 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "GND"))
    (pad "11" smd rect (at 7.35 7.5 90) (size 3.5 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "GND"))
    (model "${KISYS3DMOD}/Connectors.3dshapes/microSD_Card_Receptacle_Wuerth_693072010801.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xse-sdlogger:LED_0805_HandSoldering" (layer "F.Cu")
    (at 140.1274 91.0336 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "D2" (at 0 -1.7 180) (layer "F.SilkS"))
    (fp_text value "RED" (at 0 1.75 180) (layer "F.Fab") hide)
    (pad "1" smd rect (at -1.35 0 180) (size 1.5 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "GND"))
    (pad "2" smd rect (at 1.35 0 180) (size 1.5 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(D2-Pad2)"))
    (model "${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xse-sdlogger:C_0805_HandSoldering" (layer "B.Cu")
    (at 139.0342 99.361766)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference "C6" (at -3.3982 -0.047766 180) (layer "B.SilkS"))
    (fp_text value "0.1" (at 0 -1.75 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.75 180) (layer "B.Fab"))
    (pad "1" smd rect (at -1.25 0) (size 1.5 1.25) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "GND"))
    (pad "2" smd rect (at 1.25 0) (size 1.5 1.25) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "Net-(C6-Pad2)"))
    (model "Capacitors_SMD.3dshapes/C_0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xse-sdlogger:TQFP-44_10x10mm_Pitch0.8mm" (layer "B.Cu")
    (at 148.979 102.053 180)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference "U1" (at 0 7.45) (layer "B.SilkS") hide)
    (fp_text value "ATmega644P-20AU" (at 0 -7.45) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect (at -5.7 4 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "Net-(J2-Pad1)"))
    (pad "2" smd rect (at -5.7 3.2 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "Net-(J2-Pad2)"))
    (pad "3" smd rect (at -5.7 2.4 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "Net-(J2-Pad3)"))
    (pad "4" smd rect (at -5.7 1.6 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "Net-(C1-Pad2)"))
    (pad "5" smd rect (at -5.7 0.8 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "+3V3"))
    (pad "6" smd rect (at -5.7 0 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "GND"))
    (pad "7" smd rect (at -5.7 -0.8 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "Net-(C8-Pad2)"))
    (pad "8" smd rect (at -5.7 -1.6 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "Net-(C7-Pad2)"))
    (pad "9" smd rect (at -5.7 -2.4 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "Net-(R3-Pad2)"))
    (pad "10" smd rect (at -5.7 -3.2 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "Net-(J1-Pad3)"))
    (pad "11" smd rect (at -5.7 -4 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "Net-(J3-Pad1)"))
    (pad "12" smd rect (at -4 -5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "Net-(J3-Pad2)"))
    (pad "13" smd rect (at -3.2 -5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "Net-(U1-Pad13)"))
    (pad "14" smd rect (at -2.4 -5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "Net-(U1-Pad14)"))
    (pad "15" smd rect (at -1.6 -5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "Net-(U1-Pad15)"))
    (pad "16" smd rect (at -0.8 -5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "Net-(U1-Pad16)"))
    (pad "17" smd rect (at 0 -5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "+3V3"))
    (pad "18" smd rect (at 0.8 -5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "GND"))
    (pad "19" smd rect (at 1.6 -5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "Net-(J4-Pad2)"))
    (pad "20" smd rect (at 2.4 -5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "Net-(J4-Pad1)"))
    (pad "21" smd rect (at 3.2 -5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "Net-(J6-Pad10)"))
    (pad "22" smd rect (at 4 -5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "Net-(U1-Pad22)"))
    (pad "23" smd rect (at 5.7 -4 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "Net-(U1-Pad23)"))
    (pad "24" smd rect (at 5.7 -3.2 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "Net-(U1-Pad24)"))
    (pad "25" smd rect (at 5.7 -2.4 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "Net-(U1-Pad25)"))
    (pad "26" smd rect (at 5.7 -1.6 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "Net-(U1-Pad26)"))
    (pad "27" smd rect (at 5.7 -0.8 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "Net-(C6-Pad2)"))
    (pad "28" smd rect (at 5.7 0 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "GND"))
    (pad "29" smd rect (at 5.7 0.8 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "Net-(C6-Pad2)"))
    (pad "30" smd rect (at 5.7 1.6 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 34 "Net-(U1-Pad30)"))
    (pad "31" smd rect (at 5.7 2.4 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "Net-(U1-Pad31)"))
    (pad "32" smd rect (at 5.7 3.2 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "Net-(U1-Pad32)"))
    (pad "33" smd rect (at 5.7 4 180) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "Net-(U1-Pad33)"))
    (pad "34" smd rect (at 4 5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "Net-(J5-Pad4)"))
    (pad "35" smd rect (at 3.2 5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "Net-(J5-Pad3)"))
    (pad "36" smd rect (at 2.4 5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "Net-(J5-Pad2)"))
    (pad "37" smd rect (at 1.6 5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "Net-(J5-Pad1)"))
    (pad "38" smd rect (at 0.8 5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "+3V3"))
    (pad "39" smd rect (at 0 5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "GND"))
    (pad "40" smd rect (at -0.8 5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "Net-(R1-Pad1)"))
    (pad "41" smd rect (at -1.6 5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "Net-(R2-Pad1)"))
    (pad "42" smd rect (at -2.4 5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "Net-(U1-Pad42)"))
    (pad "43" smd rect (at -3.2 5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "Net-(U1-Pad43)"))
    (pad "44" smd rect (at -4 5.7 90) (size 1.5 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "Net-(J6-Pad2)"))
    (model "${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-44_10x10mm_Pitch0.8mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xse-sdlogger:R_0603_HandSoldering" (layer "B.Cu")
    (at 138.7342 104.749698)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference "R3" (at -2.9712 -0.101698 180) (layer "B.SilkS"))
    (fp_text value "100" (at -9.1942 -0.101698 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab") hide)
    (pad "1" smd rect (at -1.1 0) (size 1.2 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "Net-(J1-Pad2)"))
    (pad "2" smd rect (at 1.1 0) (size 1.2 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "Net-(R3-Pad2)"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xse-sdlogger:C_0805_HandSoldering" (layer "B.Cu")
    (at 139.0342 96.6978)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference "C1" (at -3.3982 0.0762 180) (layer "B.SilkS"))
    (fp_text value "0.1" (at -9.2402 0.0762 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.75 180) (layer "B.Fab") hide)
    (pad "1" smd rect (at -1.25 0) (size 1.5 1.25) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "Net-(C1-Pad1)"))
    (pad "2" smd rect (at 1.25 0) (size 1.5 1.25) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "Net-(C1-Pad2)"))
    (model "Capacitors_SMD.3dshapes/C_0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xse-sdlogger:R_0603_HandSoldering" (layer "B.Cu")
    (at 137.6774 91.0336)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference "R2" (at 0 1.45 180) (layer "B.SilkS"))
    (fp_text value "1K" (at -8.1374 -0.1016 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab") hide)
    (pad "1" smd rect (at -1.1 0) (size 1.2 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "Net-(R2-Pad1)"))
    (pad "2" smd rect (at 1.1 0) (size 1.2 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "Net-(D2-Pad2)"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xse-sdlogger:R_0603_HandSoldering" (layer "B.Cu")
    (at 158.875 91.0336 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference "R1" (at -0.0128 -1.4986) (layer "B.SilkS"))
    (fp_text value "10K" (at -9.781 0.1016) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect (at -1.1 0 180) (size 1.2 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "Net-(R1-Pad1)"))
    (pad "2" smd rect (at 1.1 0 180) (size 1.2 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "Net-(D1-Pad2)"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xse-sdlogger:C_0603_HandSoldering" (layer "B.Cu")
    (at 151.257 110.633 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.889) (layer "B.SilkS"))
    (fp_text value "4.7" (at -0.127 -7.477) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.25) (layer "B.Fab") hide)
    (pad "1" smd rect (at -0.95 0 180) (size 1.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "GND"))
    (pad "2" smd rect (at 0.95 0 180) (size 1.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "Net-(C5-Pad2)"))
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xse-sdlogger:L_0603_HandSoldering" (layer "B.Cu")
    (at 145.126 110.633)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference "L1" (at 0 1.9 180) (layer "B.SilkS"))
    (fp_text value "22uH" (at 0 7.223 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab") hide)
    (pad "1" smd rect (at -1.1 0) (size 1.2 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "+3V3"))
    (pad "2" smd rect (at 1.1 0) (size 1.2 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "Net-(C5-Pad2)"))
    (model "${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xse-sdlogger:C_0805_HandSoldering" (layer "B.Cu")
    (at 139.0342 114.4016)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference "C2" (at -3.3982 -0.1016 180) (layer "B.SilkS"))
    (fp_text value "1" (at -9.2402 0.1524 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.75 180) (layer "B.Fab") hide)
    (pad "1" smd rect (at -1.25 0) (size 1.5 1.25) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "GND"))
    (pad "2" smd rect (at 1.25 0) (size 1.5 1.25) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "+3V3"))
    (model "Capacitors_SMD.3dshapes/C_0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xse-sdlogger:C_0805_HandSoldering" (layer "B.Cu")
    (at 139.0342 111.73763)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference "C3" (at -3.3982 0.02237 180) (layer "B.SilkS"))
    (fp_text value "0.1" (at -9.4942 0.27637 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.75 180) (layer "B.Fab") hide)
    (pad "1" smd rect (at -1.25 0) (size 1.5 1.25) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "GND"))
    (pad "2" smd rect (at 1.25 0) (size 1.5 1.25) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "+3V3"))
    (model "Capacitors_SMD.3dshapes/C_0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xse-sdlogger:SOT-23-5_HandSoldering" (layer "B.Cu")
    (at 139.1666 108.158664)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference "U2" (at 0 2.9) (layer "B.SilkS") hide)
    (fp_text value "TC1015-3.3VCT713" (at -15.490058 0.06604) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "B.Fab"))
    (pad "1" smd rect (at -1.35 0.95) (size 1.56 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 46 "VIN"))
    (pad "2" smd rect (at -1.35 0) (size 1.56 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "GND"))
    (pad "3" smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 46 "VIN"))
    (pad "4" smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "Net-(U2-Pad4)"))
    (pad "5" smd rect (at 1.35 0.95) (size 1.56 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "+3V3"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xse-sdlogger:L_0805_HandSoldering" (layer "B.Cu")
    (at 139.1842 102.140732)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "L2" (at -3.5482 -0.032732 180) (layer "B.SilkS"))
    (fp_text value "10uH" (at -10.1522 -0.032732 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab") hide)
    (pad "1" smd rect (at -1.35 0) (size 1.5 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "+3V3"))
    (pad "2" smd rect (at 1.35 0) (size 1.5 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "Net-(C6-Pad2)"))
    (model "${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xse-sdlogger:C_0603_HandSoldering" (layer "B.Cu")
    (at 159.1755 101.705692 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference "C8" (at -3.0035 -0.021308) (layer "B.SilkS"))
    (fp_text value "22pF" (at -9.9885 0.105692) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.25) (layer "B.Fab") hide)
    (pad "1" smd rect (at -0.95 0 180) (size 1.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "GND"))
    (pad "2" smd rect (at 0.95 0 180) (size 1.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "Net-(C8-Pad2)"))
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xse-sdlogger:R_0603_HandSoldering" (layer "B.Cu")
    (at 159.0255 112.26148)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference "R5" (at 3.1535 0.00652 180) (layer "B.SilkS"))
    (fp_text value "1K" (at 8.8685 -0.24748 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab"))
    (pad "1" smd rect (at -1.1 0) (size 1.2 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "+3V3"))
    (pad "2" smd rect (at 1.1 0) (size 1.2 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "Net-(J4-Pad2)"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xse-sdlogger:R_0603_HandSoldering" (layer "B.Cu")
    (at 159.0255 110.05378)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference "R6" (at 2.9503 0.0339) (layer "B.SilkS"))
    (fp_text value "1K" (at 8.683338 0.00442) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd rect (at -1.1 0) (size 1.2 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "+3V3"))
    (pad "2" smd rect (at 1.1 0) (size 1.2 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "Net-(J4-Pad1)"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xse-sdlogger:R_0603_HandSoldering" (layer "B.Cu")
    (at 159.0155 97.0153 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference "R4" (at -3.1635 -0.0127) (layer "B.SilkS"))
    (fp_text value "10K" (at -10.0215 -0.0127) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd rect (at -1.1 0 180) (size 1.2 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "+3V3"))
    (pad "2" smd rect (at 1.1 0 180) (size 1.2 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "Net-(C1-Pad2)"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xse-sdlogger:IQD_3.2x2.5mm" (layer "B.Cu")
    (at 158.8734 104.808388 180)
    (descr "SMD Crystal SERIES SMD7050/4 https://www.foxonline.com/pdfs/FQ7050.pdf, 7.0x5.0mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference "Y1" (at -3.05988 0.02657) (layer "B.SilkS") hide)
    (fp_text value "LFXTAL036338" (at -13.2402 0.007988) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0.07448 -0.03947) (layer "B.Fab") hide)
    (pad "1" smd rect (at 1.1 0.8 180) (size 1.4 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "Net-(C8-Pad2)"))
    (pad "2" smd rect (at -1.1 0.8 180) (size 1.4 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "GND"))
    (pad "3" smd rect (at -1.1 -0.8 180) (size 1.4 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "Net-(C7-Pad2)"))
    (pad "4" smd rect (at 1.1 -0.8 180) (size 1.4 1.15) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "GND"))
    (model "${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_7050-4pin_7.0x5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xse-sdlogger:C_0805_HandSoldering" (layer "B.Cu")
    (at 158.7255 99.392996 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference "C4" (at -3.4535 -0.048004) (layer "B.SilkS"))
    (fp_text value "0.1" (at -9.9305 0.078996) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.75) (layer "B.Fab") hide)
    (pad "1" smd rect (at -1.25 0 180) (size 1.5 1.25) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "GND"))
    (pad "2" smd rect (at 1.25 0 180) (size 1.5 1.25) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "+3V3"))
    (model "Capacitors_SMD.3dshapes/C_0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "xse-sdlogger:C_0603_HandSoldering" (layer "B.Cu")
    (at 159.1755 107.911084)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference "C7" (at 3.0035 0.038916 180) (layer "B.SilkS"))
    (fp_text value "22pF" (at 10.2425 0.165916 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.25 180) (layer "B.Fab"))
    (pad "1" smd rect (at -0.95 0) (size 1.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "GND"))
    (pad "2" smd rect (at 0.95 0) (size 1.2 0.75) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "Net-(C7-Pad2)"))
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 131.6434 89.835) (end 131.6434 116.814)
    (layer "Edge.Cuts"))
  (gr_line (start 166.2434 89.835) (end 166.2434 116.814)
    (layer "Edge.Cuts"))
  (gr_line (start 131.6434 116.814) (end 166.2434 116.814)
    (layer "Edge.Cuts"))
  (gr_line (start 131.6434 89.835) (end 166.2434 89.835)
    (layer "Edge.Cuts"))
  (gr_text "GND" (at 137.080628 114.6955) (layer "F.SilkS"))
  (gr_text "VIN" (at 136.747295 109.6155) (layer "F.SilkS"))
  (gr_text "RX" (at 136.533009 104.5355) (layer "F.SilkS"))
  (gr_text "TX" (at 136.413962 107.0755) (layer "F.SilkS"))
  (gr_text "TX2" (at 136.890152 95.2755) (layer "F.SilkS"))
  (gr_text "GND" (at 137.080628 112.1555) (layer "F.SilkS"))
  (gr_text "DTR" (at 136.937771 101.9955) (layer "F.SilkS"))
  (gr_text "RX2" (at 137.0092 92.7355) (layer "F.SilkS"))
  (gr_text "GND" (at 137.080628 97.8155) (layer "F.SilkS"))
  (gr_text "A0" (at 161.074 91.9988) (layer "F.SilkS"))
  (gr_text "A1" (at 161.074 94.2213) (layer "F.SilkS"))
  (gr_text "A2" (at 161.074 96.6597) (layer "F.SilkS"))
  (gr_text "A3" (at 161.074 99.6061) (layer "F.SilkS"))
  (gr_text "GND" (at 160.454952 102.0826) (layer "F.SilkS"))
  (gr_text "SDA" (at 160.574 107.2515) (layer "F.SilkS"))
  (gr_text "SCL" (at 160.597809 109.601) (layer "F.SilkS"))
  (gr_text "3.3V" (at 160.359714 112.2553) (layer "F.SilkS"))
  (gr_text "GND" (at 160.454952 114.8969) (layer "F.SilkS"))
  (gr_text "MISO" (at 145.62986 112.9792) (layer "F.SilkS"))
  (gr_text "SCK" (at 148.16986 112.9792) (layer "F.SilkS"))
  (gr_text "RST" (at 150.70986 112.9792) (layer "F.SilkS"))
  (gr_text "3.3V" (at 153.24986 112.9792) (layer "F.SilkS"))
  (gr_text "GND" (at 155.78986 112.9792) (layer "F.SilkS"))
  (gr_text "MOSI" (at 143.08986 112.9792) (layer "F.SilkS"))
  (gr_text "XSE SDLogger V1.3" (at 148.9473 111.0932) (layer "F.Mask"))
  (zone (net 45) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.2176 89.8398)
        (xy 166.243 116.8146)
        (xy 131.6482 116.7892)
        (xy 131.5974 89.8144)
      )
    )
  )
)
